                                                                                                         The DIGITAL logo is a trademark of Digital Equipment Corporation.

Copyright 1997 Digital Equipment Cor poration

EK˘SWXES˘IG. A01

                                                      Installing a Ferrite Bead on a Host Bus Cable

                                                                                                            To suppress e lectromagn etic interfere nce  (EMI) in a

                                                                                                      SW600 -ser ies ca binet, follow th ese instru ctions to place

a ferr ite  bea d on  the host bus cable.

CAUTION: Both Ultra SCSI bus controllers require a ferrite bead on their host bus cables to ensure com pliance with CE-mark and

FCC Class A standards. DIG ITAL does not authorize the operation of any Ultra SCSI cabinet subsystem without both beads installed  in

the proper manner.

To install the ferrite be ad...

1. Remove the ferrite bead from the plastic bag.

2. Snap the ferrite bead on the host bus cable within one inch of the controller as shown in Figure 1.

Figure  1.   Array Controller with Ferrite Bead on Host Bus Cable